 -- Copyright (C) 1991-2004 Altera Corporation
 -- Any  megafunction  design,  and related netlist (encrypted  or  decrypted),
 -- support information,  device programming or simulation file,  and any other
 -- associated  documentation or information  provided by  Altera  or a partner
 -- under  Altera's   Megafunction   Partnership   Program  may  be  used  only
 -- to program  PLD  devices (but not masked  PLD  devices) from  Altera.   Any
 -- other  use  of such  megafunction  design,  netlist,  support  information,
 -- device programming or simulation file,  or any other  related documentation
 -- or information  is prohibited  for  any  other purpose,  including, but not
 -- limited to  modification,  reverse engineering,  de-compiling, or use  with
 -- any other  silicon devices,  unless such use is  explicitly  licensed under
 -- a separate agreement with  Altera  or a megafunction partner.  Title to the
 -- intellectual property,  including patents,  copyrights,  trademarks,  trade
 -- secrets,  or maskworks,  embodied in any such megafunction design, netlist,
 -- support  information,  device programming or simulation file,  or any other
 -- related documentation or information provided by  Altera  or a megafunction
 -- partner, remains with Altera, the megafunction partner, or their respective
 -- licensors. No other licenses, including any licenses needed under any third
 -- party's intellectual property, are provided herein.
 ------------------------------------------------------------------------------



 ------------------------------------------------------------------------------
 -- NC         : No Connect. This pin has no internal connection to the device.
 -- VCC_INT    : Dedicated power pin, which MUST be connected to VCC  (5.0V).
 -- VCC_IO     : Dedicated power pin, which MUST be connected to VCC  (Refer to
 --              the table below for voltage).
 -- GND        : Dedicated ground pin, which MUST be connected to GND.
 -- GND+       : Unused input. This pin should be connected to GND. It may also
 --              be connected  to a  valid signal  on the board  (low, high, or
 --              toggling)  if that signal is required for a different revision
 --              of the design.
 -- GND*       : Unused  I/O  pin.   This pin can either be left unconnected or
 --              connected to GND.  Connecting this pin to GND will improve the
 --              device's immunity to noise.
 ------------------------------------------------------------------------------


Quartus II Version 4.0 Build 214 3/25/2004 Service Pack 1 SJ Full Version
CHIP  "tutor2"  ASSIGNED TO AN: EPF10K70RC240-4

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
TCK                          : 1         : input  :                   :         :           :                
CONF_DONE                    : 2         : bidir  :                   :         :           :                
nCEO                         : 3         : output :                   :         :           :                
TDO                          : 4         : output :                   :         :           :                
VCC_INT                      : 5         : power  :                   : 5.0V    :           :                
MSD_SEG_A                    : 6         : output : TTL               :         :           : Y              
MSD_SEG_B                    : 7         : output : TTL               :         :           : Y              
MSD_SEG_C                    : 8         : output : TTL               :         :           : Y              
MSD_SEG_D                    : 9         : output : TTL               :         :           : Y              
GND_INT                      : 10        : gnd    :                   :         :           :                
MSD_SEG_E                    : 11        : output : TTL               :         :           : Y              
MSD_SEG_F                    : 12        : output : TTL               :         :           : Y              
MSD_SEG_G                    : 13        : output : TTL               :         :           : Y              
MSD_SEG_DP                   : 14        : output : TTL               :         :           : Y              
GND*                         : 15        :        :                   :         :           :                
VCC_INT                      : 16        : power  :                   : 5.0V    :           :                
LSD_SEG_A                    : 17        : output : TTL               :         :           : Y              
LSD_SEG_B                    : 18        : output : TTL               :         :           : Y              
LSD_SEG_C                    : 19        : output : TTL               :         :           : Y              
LSD_SEG_D                    : 20        : output : TTL               :         :           : Y              
LSD_SEG_E                    : 21        : output : TTL               :         :           : Y              
GND_INT                      : 22        : gnd    :                   :         :           :                
LSD_SEG_F                    : 23        : output : TTL               :         :           : Y              
LSD_SEG_G                    : 24        : output : TTL               :         :           : Y              
LSD_SEG_DP                   : 25        : output : TTL               :         :           : Y              
GND*                         : 26        :        :                   :         :           :                
VCC_INT                      : 27        : power  :                   : 5.0V    :           :                
PB1                          : 28        : input  : TTL               :         :           : Y              
PB2                          : 29        : input  : TTL               :         :           : Y              
GND*                         : 30        :        :                   :         :           :                
GND*                         : 31        :        :                   :         :           :                
GND_INT                      : 32        : gnd    :                   :         :           :                
GND*                         : 33        :        :                   :         :           :                
GND*                         : 34        :        :                   :         :           :                
GND*                         : 35        :        :                   :         :           :                
GND*                         : 36        :        :                   :         :           :                
VCC_INT                      : 37        : power  :                   : 5.0V    :           :                
GND*                         : 38        :        :                   :         :           :                
GND*                         : 39        :        :                   :         :           :                
GND*                         : 40        :        :                   :         :           :                
GND*                         : 41        :        :                   :         :           :                
GND_INT                      : 42        : gnd    :                   :         :           :                
GND*                         : 43        :        :                   :         :           :                
GND*                         : 44        :        :                   :         :           :                
GND*                         : 45        :        :                   :         :           :                
GND*                         : 46        :        :                   :         :           :                
VCC_INT                      : 47        : power  :                   : 5.0V    :           :                
GND*                         : 48        :        :                   :         :           :                
GND*                         : 49        :        :                   :         :           :                
GND*                         : 50        :        :                   :         :           :                
GND*                         : 51        :        :                   :         :           :                
GND_INT                      : 52        : gnd    :                   :         :           :                
GND*                         : 53        :        :                   :         :           :                
GND*                         : 54        :        :                   :         :           :                
GND*                         : 55        :        :                   :         :           :                
GND*                         : 56        :        :                   :         :           :                
VCC_INT                      : 57        : power  :                   : 5.0V    :           :                
TMS                          : 58        : input  :                   :         :           :                
TRST                         : 59        : input  :                   :         :           :                
nSTATUS                      : 60        : bidir  :                   :         :           :                
GND*                         : 61        :        :                   :         :           :                
GND*                         : 62        :        :                   :         :           :                
GND*                         : 63        :        :                   :         :           :                
GND*                         : 64        :        :                   :         :           :                
GND*                         : 65        :        :                   :         :           :                
GND*                         : 66        :        :                   :         :           :                
GND*                         : 67        :        :                   :         :           :                
GND*                         : 68        :        :                   :         :           :                
GND_INT                      : 69        : gnd    :                   :         :           :                
GND*                         : 70        :        :                   :         :           :                
GND*                         : 71        :        :                   :         :           :                
GND*                         : 72        :        :                   :         :           :                
GND*                         : 73        :        :                   :         :           :                
GND*                         : 74        :        :                   :         :           :                
GND*                         : 75        :        :                   :         :           :                
GND*                         : 76        :        :                   :         :           :                
VCC_INT                      : 77        : power  :                   : 5.0V    :           :                
GND*                         : 78        :        :                   :         :           :                
GND*                         : 79        :        :                   :         :           :                
GND*                         : 80        :        :                   :         :           :                
GND*                         : 81        :        :                   :         :           :                
GND*                         : 82        :        :                   :         :           :                
GND*                         : 83        :        :                   :         :           :                
GND*                         : 84        :        :                   :         :           :                
GND_INT                      : 85        : gnd    :                   :         :           :                
GND*                         : 86        :        :                   :         :           :                
GND*                         : 87        :        :                   :         :           :                
GND*                         : 88        :        :                   :         :           :                
VCC_INT                      : 89        : power  :                   : 5.0V    :           :                
GND+                         : 90        :        :                   :         :           :                
GND+                         : 91        :        :                   :         :           :                
GND+                         : 92        :        :                   :         :           :                
GND_INT                      : 93        : gnd    :                   :         :           :                
GND*                         : 94        :        :                   :         :           :                
GND*                         : 95        :        :                   :         :           :                
VCC_INT                      : 96        : power  :                   : 5.0V    :           :                
GND*                         : 97        :        :                   :         :           :                
GND*                         : 98        :        :                   :         :           :                
GND*                         : 99        :        :                   :         :           :                
GND*                         : 100       :        :                   :         :           :                
GND*                         : 101       :        :                   :         :           :                
GND*                         : 102       :        :                   :         :           :                
GND*                         : 103       :        :                   :         :           :                
GND_INT                      : 104       : gnd    :                   :         :           :                
GND*                         : 105       :        :                   :         :           :                
GND*                         : 106       :        :                   :         :           :                
GND*                         : 107       :        :                   :         :           :                
GND*                         : 108       :        :                   :         :           :                
GND*                         : 109       :        :                   :         :           :                
GND*                         : 110       :        :                   :         :           :                
GND*                         : 111       :        :                   :         :           :                
VCC_INT                      : 112       : power  :                   : 5.0V    :           :                
GND*                         : 113       :        :                   :         :           :                
GND*                         : 114       :        :                   :         :           :                
GND*                         : 115       :        :                   :         :           :                
GND*                         : 116       :        :                   :         :           :                
GND*                         : 117       :        :                   :         :           :                
GND*                         : 118       :        :                   :         :           :                
GND*                         : 119       :        :                   :         :           :                
GND*                         : 120       :        :                   :         :           :                
nCONFIG                      : 121       : input  :                   :         :           :                
VCC_INT                      : 122       : power  :                   : 5.0V    :           :                
MSEL1                        : 123       : input  :                   :         :           :                
MSEL0                        : 124       : input  :                   :         :           :                
GND_INT                      : 125       : gnd    :                   :         :           :                
GND*                         : 126       :        :                   :         :           :                
GND*                         : 127       :        :                   :         :           :                
GND*                         : 128       :        :                   :         :           :                
GND*                         : 129       :        :                   :         :           :                
VCC_INT                      : 130       : power  :                   : 5.0V    :           :                
GND*                         : 131       :        :                   :         :           :                
GND*                         : 132       :        :                   :         :           :                
GND*                         : 133       :        :                   :         :           :                
GND*                         : 134       :        :                   :         :           :                
GND_INT                      : 135       : gnd    :                   :         :           :                
GND*                         : 136       :        :                   :         :           :                
GND*                         : 137       :        :                   :         :           :                
GND*                         : 138       :        :                   :         :           :                
GND*                         : 139       :        :                   :         :           :                
VCC_INT                      : 140       : power  :                   : 5.0V    :           :                
GND*                         : 141       :        :                   :         :           :                
GND*                         : 142       :        :                   :         :           :                
GND*                         : 143       :        :                   :         :           :                
GND*                         : 144       :        :                   :         :           :                
GND_INT                      : 145       : gnd    :                   :         :           :                
GND*                         : 146       :        :                   :         :           :                
GND*                         : 147       :        :                   :         :           :                
GND*                         : 148       :        :                   :         :           :                
GND*                         : 149       :        :                   :         :           :                
VCC_INT                      : 150       : power  :                   : 5.0V    :           :                
GND*                         : 151       :        :                   :         :           :                
GND*                         : 152       :        :                   :         :           :                
GND*                         : 153       :        :                   :         :           :                
GND*                         : 154       :        :                   :         :           :                
GND_INT                      : 155       : gnd    :                   :         :           :                
GND*                         : 156       :        :                   :         :           :                
GND*                         : 157       :        :                   :         :           :                
GND*                         : 158       :        :                   :         :           :                
GND*                         : 159       :        :                   :         :           :                
VCC_INT                      : 160       : power  :                   : 5.0V    :           :                
GND*                         : 161       :        :                   :         :           :                
GND*                         : 162       :        :                   :         :           :                
GND*                         : 163       :        :                   :         :           :                
GND*                         : 164       :        :                   :         :           :                
GND_INT                      : 165       : gnd    :                   :         :           :                
GND*                         : 166       :        :                   :         :           :                
GND*                         : 167       :        :                   :         :           :                
GND*                         : 168       :        :                   :         :           :                
GND*                         : 169       :        :                   :         :           :                
VCC_INT                      : 170       : power  :                   : 5.0V    :           :                
GND*                         : 171       :        :                   :         :           :                
GND*                         : 172       :        :                   :         :           :                
GND*                         : 173       :        :                   :         :           :                
GND*                         : 174       :        :                   :         :           :                
GND*                         : 175       :        :                   :         :           :                
GND_INT                      : 176       : gnd    :                   :         :           :                
TDI                          : 177       : input  :                   :         :           :                
nCE                          : 178       : input  :                   :         :           :                
DCLK                         : 179       : bidir  :                   :         :           :                
DATA0                        : 180       : input  :                   :         :           :                
GND*                         : 181       :        :                   :         :           :                
GND*                         : 182       :        :                   :         :           :                
GND*                         : 183       :        :                   :         :           :                
GND*                         : 184       :        :                   :         :           :                
GND*                         : 185       :        :                   :         :           :                
GND*                         : 186       :        :                   :         :           :                
GND*                         : 187       :        :                   :         :           :                
GND*                         : 188       :        :                   :         :           :                
VCC_INT                      : 189       : power  :                   : 5.0V    :           :                
GND*                         : 190       :        :                   :         :           :                
GND*                         : 191       :        :                   :         :           :                
GND*                         : 192       :        :                   :         :           :                
GND*                         : 193       :        :                   :         :           :                
GND*                         : 194       :        :                   :         :           :                
GND*                         : 195       :        :                   :         :           :                
GND*                         : 196       :        :                   :         :           :                
GND_INT                      : 197       : gnd    :                   :         :           :                
GND*                         : 198       :        :                   :         :           :                
GND*                         : 199       :        :                   :         :           :                
GND*                         : 200       :        :                   :         :           :                
GND*                         : 201       :        :                   :         :           :                
GND*                         : 202       :        :                   :         :           :                
GND*                         : 203       :        :                   :         :           :                
GND*                         : 204       :        :                   :         :           :                
VCC_INT                      : 205       : power  :                   : 5.0V    :           :                
GND*                         : 206       :        :                   :         :           :                
GND*                         : 207       :        :                   :         :           :                
GND*                         : 208       :        :                   :         :           :                
GND*                         : 209       :        :                   :         :           :                
GND+                         : 210       :        :                   :         :           :                
GND+                         : 211       :        :                   :         :           :                
GND+                         : 212       :        :                   :         :           :                
GND*                         : 213       :        :                   :         :           :                
GND*                         : 214       :        :                   :         :           :                
GND*                         : 215       :        :                   :         :           :                
GND_INT                      : 216       : gnd    :                   :         :           :                
GND*                         : 217       :        :                   :         :           :                
GND*                         : 218       :        :                   :         :           :                
GND*                         : 219       :        :                   :         :           :                
GND*                         : 220       :        :                   :         :           :                
GND*                         : 221       :        :                   :         :           :                
GND*                         : 222       :        :                   :         :           :                
GND*                         : 223       :        :                   :         :           :                
VCC_INT                      : 224       : power  :                   : 5.0V    :           :                
GND*                         : 225       :        :                   :         :           :                
GND*                         : 226       :        :                   :         :           :                
GND*                         : 227       :        :                   :         :           :                
GND*                         : 228       :        :                   :         :           :                
GND*                         : 229       :        :                   :         :           :                
GND*                         : 230       :        :                   :         :           :                
GND*                         : 231       :        :                   :         :           :                
GND_INT                      : 232       : gnd    :                   :         :           :                
GND*                         : 233       :        :                   :         :           :                
GND*                         : 234       :        :                   :         :           :                
GND*                         : 235       :        :                   :         :           :                
GND*                         : 236       :        :                   :         :           :                
GND*                         : 237       :        :                   :         :           :                
GND*                         : 238       :        :                   :         :           :                
GND*                         : 239       :        :                   :         :           :                
GND*                         : 240       :        :                   :         :           :                
