# Copyright (C) 1991-2004 Altera Corporation
# Any  megafunction  design,  and related netlist (encrypted  or  decrypted),
# support information,  device programming or simulation file,  and any other
# associated  documentation or information  provided by  Altera  or a partner
# under  Altera's   Megafunction   Partnership   Program  may  be  used  only
# to program  PLD  devices (but not masked  PLD  devices) from  Altera.   Any
# other  use  of such  megafunction  design,  netlist,  support  information,
# device programming or simulation file,  or any other  related documentation
# or information  is prohibited  for  any  other purpose,  including, but not
# limited to  modification,  reverse engineering,  de-compiling, or use  with
# any other  silicon devices,  unless such use is  explicitly  licensed under
# a separate agreement with  Altera  or a megafunction partner.  Title to the
# intellectual property,  including patents,  copyrights,  trademarks,  trade
# secrets,  or maskworks,  embodied in any such megafunction design, netlist,
# support  information,  device programming or simulation file,  or any other
# related documentation or information provided by  Altera  or a megafunction
# partner, remains with Altera, the megafunction partner, or their respective
# licensors. No other licenses, including any licenses needed under any third
# party's intellectual property, are provided herein.


# The default values for assignments are stored in the file
#		assignment_defaults.qdf

# Altera recommends that you do not modify this file. This
# file is updated automatically by the Quartus II software
# and any changes you make may be lost or overwritten.


# Project-Wide Assignments
# ========================
set_global_assignment -name ORIGINAL_QUARTUS_VERSION "4.0 SP1"
set_global_assignment -name PROJECT_CREATION_TIME_DATE "09:41:48  JUNE 17, 2004"
set_global_assignment -name LAST_QUARTUS_VERSION "4.0 SP1"
set_global_assignment -name BDF_FILE src/tutor3.bdf

# Pin & Location Assignments
# ==========================
set_location_assignment PIN_91 -to Clock_25Mhz
set_location_assignment PIN_29 -to PB2
set_location_assignment PIN_28 -to PB1
set_location_assignment PIN_6 -to MSD_SEG_A
set_location_assignment PIN_7 -to MSD_SEG_B
set_location_assignment PIN_8 -to MSD_SEG_C
set_location_assignment PIN_9 -to MSD_SEG_D
set_location_assignment PIN_11 -to MSD_SEG_E
set_location_assignment PIN_12 -to MSD_SEG_F
set_location_assignment PIN_13 -to MSD_SEG_G
set_location_assignment PIN_14 -to MSD_SEG_DP
set_location_assignment PIN_17 -to LSD_SEG_A
set_location_assignment PIN_18 -to LSD_SEG_B
set_location_assignment PIN_19 -to LSD_SEG_C
set_location_assignment PIN_20 -to LSD_SEG_D
set_location_assignment PIN_21 -to LSD_SEG_E
set_location_assignment PIN_23 -to LSD_SEG_F
set_location_assignment PIN_24 -to LSD_SEG_G
set_location_assignment PIN_25 -to LSD_SEG_DP

# Analysis & Synthesis Assignments
# ================================
set_global_assignment -name FAMILY FLEX10K
set_global_assignment -name TOP_LEVEL_ENTITY tutor3
set_global_assignment -name USER_LIBRARIES "c:\\qdesigns\\uplib"

# Fitter Assignments
# ==================
set_global_assignment -name DEVICE "EPF10K70RC240-4"
